(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "UIAPDUINO-PRO-MICRO-CH32V003-V1DOT4"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 18.542 0)
		)
		(property "Value" "UIAPDUINO-PRO-MICRO-CH32V003-V1DOT4"
			(at -15.24 -17.78 0)
		)
		(property "Footprint" "UIAP-Devices:UIAPDUINO-PRO-MICRO-CH32V003-V1DOT4"
			(at 0.762 3.81 0)
		)
		(property "Datasheet" "https://www.uiap.jp/en/uiapduino/pro-micro/ch32v003/v1dot4"
			(at 0 0 0)
		)
		(property "Description" "Specifications: Pins 7, 8, and 9 are present on both sides., Version: 1.0.0, 2025/06/19, Design: Yuuki Umeta, CC BY-SA 4.0, https://creativecommons.org/licenses/by-sa/4.0/"
			(at 0 0 0)
		)
		(property "ki_keywords" "UIAPduino Pro Micro CH32V003 V1.4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UIAPDUINO-PRO-MICRO-CH32V003-V1DOT4*"
			(at 0 0 0)
		)
		(symbol "UIAPDUINO-PRO-MICRO-CH32V003-V1DOT4_0_1")
		(symbol "UIAPDUINO-PRO-MICRO-CH32V003-V1DOT4_1_0")
		(symbol "UIAPDUINO-PRO-MICRO-CH32V003-V1DOT4_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "15/A5(TX)")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "16/A6(RX)")
				(number "2")
			)
			(pin power_in line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "->3(SDA)")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "->4(SCL)")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "*2")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "*5")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "11")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "->7(SCK)")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "->8(MOSI)")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "9(MISO)")
				(number "12")
			)
			(pin power_in line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "5V")
				(number "24")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "GND")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "~{RESET}")
				(number "22")
			)
			(pin power_in line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "3V3")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "12/A3")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "*6/A2(SS)")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "0/A1")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "1/A0")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "->7(SCK)")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "9(MISO)")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "->8(MOSI)")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "10")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
)
